**Overall summary:**

**Operation:** No abnormal operating conditions during the month

**Incidents:** No incidents recorded impacting air quality

**Exceedances:** No exceedances recorded


**In-tunnel air quality data (NO2 - 15 min maximum):**

**M8 – Rozelle Interchange:**


**A screenshot of a graph

Description automatically generated**


**M4 – Rozelle Interchange:**

****

**Ambient (NO2 - 1 hour average)**

****

**Ventilation Outlet (NO2 - 1 hour average):**

****

***The data reflected in this document has undergone preliminary quality assurance checks. Validated air quality data reports are made available on the*** [***Linkt Environmental and Air Quality Reports***](https://www.linkt.com.au/using-toll-roads/safety/air-quality/sydney) ***wepbage one month after the end of the calendar month.***